( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

1. Align the bolt hole (A) on the steering joint with the groove (B) around the pinion shaft, then loosely install the lower steering joint bolt (C). Be sure that the joint bolt is securely in the groove in the pinion shaft.

1. Pull on the steering joint to make sure that the steering joint is fully seated, then tighten the lower joint bolt to the specified torque.

1. Tighten the upper steering joint bolt (D) to the specified torque.