( TL19E30A20336359401LBAT00 )

Throttle Body Cleaning

Do not insert your fingers into the installed throttle body when you turn the ignition switch to ON (II) or while the ignition switch is ON (II). If you do, you will seriously injure your fingers if the throttle valve is activated.

1. Make sure the ignition switch turned LOCK (0).

1. Check for damage to the air cleaner. If the air cleaner is damaged, replace it.

1. Remove the throttle body.

1. Clean off the carbon from the throttle valve and inside the throttle body with a paper towel soaked in throttle plate and induction cleaner.
   NOTE:
   - Remove the throttle body to clean it.
   - Be careful not to pinch your fingers.
   - To avoid removing the molybdenum coating, do not clean the bearing area of the throttle shaft (A).
   - Do not spray carburetor cleaner directly on the throttle body.
   - Use Honda genuine carburetor cleaner.

1. Install the throttle body.

1. Connect the HDS to the data link connector (DLC) (A) located under the driver's side of the dashboard.

1. Turn the ignition switch to ON (II).

1. Reset the ECM/PCM with the HDS.

1. Select the ETCS TEST in the INSPECTION MENU with the HDS.

1. Select TP POSITION CHECK and clear the throttle position (TP) learned value.

1. Turn the ignition switch to LOCK (0).

1. Turn the ignition switch to ON (II), and wait 2 seconds without pressing the accelerator pedal.

1. Do the ECM/PCM idle learn procedure.