( TL19E00B20200037701KDAT00 )

Front Lower Arm Removal/Installation

1. Clean the mating surfaces of the new compliance bushing (A) and the lower arm (B).

1. Make sure of the compliance bushing installation direction, align the bushing aligning marks with the lower arm, then press in the bushing into the lower arm using the bushing driver, the bushing receiver set (attachments A and B), and a hydraulic press.
   NOTE:
   - Press in the bushing from the bottom side of the lower arm.
   - After installation, check the protrusion (C) of the bushing outer sleeve (D) through the lower arm bushing hole (E).

1. Install the lower arm.