( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

Installation

1. Before installing the steering gearbox, make sure that no grease is on the mating surface of the steering gearbox and the front subframe. To prevent the gearbox mounting bolts from loosening after the installation, remove any grease from the bolt holes.

1. Wrap vinyl tape to the splines on the pinion shaft (A).

1. Install the EPS subharness (B) to the steering gearbox (C).