( TL19E00H1080001242DKDAT00 )

ACC Combination Switch and Distance/LKAS Switch Removal/Installation

1. Remove the driver's airbag inflator.

1. Remove the lids (A) from the steering wheel.

1. Remove the screws (A) from the steering wheel.

1. Disconnect the ACC combination switch 12P connector (A) and audio remote switch 12P connector (B).

1. Release the hook (C) and pull up the pins (D) by pulling the steering wheel, then disconnect the distance/LKAS OFF switch 7P connector (E) and HFT switch 7P connector (F).

1. Remove the screws, then remove the distance/LKAS switch (A) from the steering wheel trim (B).

1. Remove the screw and release the hook, then remove the ACC combination switch (A) from the steering wheel trim (B).

1. Install the ACC combination switch in the reverse order of removal.