( TL19E1PE10480139301KCAT00 )

A/T Valve Body and ATF Strainer Installation

1. Install a new O-ring on the ATF strainer, and install the ATF strainer on the servo body, then secure the ATF strainer with the two bolts in the bolt holes (A).

1. Install the regulator separator plate and the two dowel pins on the main valve body.

1. Install a new O-ring on the stator shaft, and install the stator shaft and the stator shaft stop.

1. Install the regulator valve body (eight bolts).

1. Install the ATF joint pipes (one bolt).

1. Install the ATF feed pipes in the regulator valve body and the servo body.