( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

1. Adjust the pinion (A) of the rear brake (B).

   -1. | Engage the gear (C) with the motor pinion by hand, and center it.
   -2. | Check the positions of the sector gear (D) and the cross-shaped hole (E) in the gear.
   -3. | Using a 8 mm hexagonal wrench, adjust the pinion of the rear brake to the sector gear and also fingers (F) around the axle to the cross-shaped hole in the gear.