( TL19E1PE10410424251KCAT00 )

A/T End Cover Installation

1. Move the selector control shaft (A) from the P position to the N position by turning the selector control shaft with the selector control lever on the torque converter side.
   NOTE: Do not squeeze the end of the selector control shaft tips together when turning the shaft. If the selector control shaft tips are squeezed together, it will cause a faulty shift position signal or position due to the play between the selector control shaft and the transmission range switch.