( TL19E00H10800040231MBAT00 )

Millimeter Wave Radar Aiming

1. Follow the onscreen instructions on the HDS to confirm the horizontal aiming is correct or to make the necessary adjustments.
   NOTE: The result of all auto aiming can be confirmed by the HDS, or when ‘‘RADAR OK'' appears on the MID, or by the brake lights illuminating. When the target is not in the range 100±2 or a tone is sounded by the vehicle when the aiming point is out of specification, or when the brake lights do not come on, the auto aiming is not completed correctly. If DTC 120, 121,122, 123, or 124 is indicated, the aiming target is not set correctly. Reset the aiming target.

1. After adjustment, confirm the MID display and the lighting of the brake lights, and finalize the horizontal aiming (End the aiming process on the HDS).

1. After aiming, clear the DTCs with the HDS.