( TL19E00J36100000000FEAT00 )

Navigation System Diagnostic Mode

Start-up procedure and Diagnostic Menu
There are two ways to enter the diagnostic mode:

1. Start the vehicle and at the globe screen connect the SCS service connector to the navigation service connector located behind the navigation unit in the trunk. The screen changes to the System Links screen automatically begins running the self-diagnostic. See the System Links section for more information.
   NOTE: When finished troubleshooting, make sure to remove the SCS service connector.