( TL19E00J32300035061FHAT00 )

Interior Light Switch Test/Replacement

With sunroof
NOTE: The interior light switch is built into the sunroof switch, and it switches the front individual map light OFF and DOOR positions.

1. Remove the front individual map lights.

1. Disconnect the sunroof switch 12P connector (A) and the map light 3P connector (B).

1. Remove the sunroof switch (C) from the map light housing.

1. At the sunroof switch 12P connector, check for continuity between the No. 9 and No. 7 terminals.
   - There should be continuity when the interior light switch is in the DOOR position.
   - There should be no continuity when the interior light switch is in the OFF position.

1. If the continuity is not as specified, replace the sunroof switch assembly.

1. Install the parts in the reverse order of removal.