( TL19E00J54260461995CBAT00 )

Fuse to Components Index - Drivwe's Under-dash Fuse/Relay Box

Driver's Under-dash Fuse/Relay Box

Fuse Number | Amps | Component(s) or Circuit(s) Protected
--- | --- | ---
1 | 7.5 A | E-pretensioner unit (With ACC), LKAS unit
2 | 7.5 A | Left headlight leveling motor *2 , ACC unit, Headlight leveling control unit (with HID), Power seat control unit (with DPMS), Millimeter wave radar (with ACC) (LHD model)
3 | 15 A | Via passenger's under-dash fuse/relay box: Windshield washer motor, Passenger's MICU
4 | 10 A | Passenger's under-dash fuse/relay box, Relay circuit board (wiper motor relay circuit)

5

7.5 A

Automatic dimming inside mirror, Gauge control module, Shift lock solenoid (A/T), Automatic lighting/rain sensor *1 , Headlight washer switch, Parking and back-up sensor switch, Parking and back-up sensor control unit, Power seat control unit (with DPMS), LKAS camera
Via passenger's under-dash fuse/relay box:
Passenger's MICU
Transmission range switch (R) (A/T), PCM (A/T), Driver's MICU (A/T), Back up-lights (A/T), Navigation unit (A/T)
Driver's MICU (M/T), Back up-lights (M/T)

6 | 7.5 A | VSA modulator-control unit, Yaw rate-lateral acceleration sensor, EPS control unit, Headlight leveling switch (without HID) *2 , Right headlight leveling motor (without HID) *2 Via relay circuit board: ACC unit, VSA modulator-control unit
7 | 15 A | Electrical load detector (ELD), Brake pedal position switch, CMP sensor A, Secondary HO2S, Engine mount control solenoid, EVAP canister purge valve, Alternator, Reverse lockout solenoid (M/T)
8 | 7.5 A | Starter solenoid (A/T), Transmission range switch (N, P) (A/T), Starter solenoid (M/T)
9 | 20 A | ECM/PCM (IG1), Fuel pump, Immobilizer-keyless control unit
10 | 10 A | ECM/PCM (VBSOL)
11 | 10 A | SRS unit
12 | 7.5 A | Front passenger's airbag cutoff indicator, OPDS unit, SRS unit
13 | ——— | Not used
14 | ——— | Not used
15 | 7.5 A | Driver's MICU (DAY LT) *3 , Not used (RHD model)

16

7.5 A

Door multiplex control unit (Power window master switch), Audio/navigation switch panel, Power mirror switch, Driver's seat heater switch, Front passenger's seat heater switch, Center subdisplay unit (LHD model), Heater control unit/climate control unit
Via under-hood fuse/relay box:
Rear window defogger switch (in the heater control unit/climate control unit), ECM/PCM (FANL), ECM/PCM (ACC)
Via Relay circuit board:
Radiator fan relay, ECM/PCM (FANH)

17 | 7.5 A | Driver's MICU
18 | 7.5 A | Center accessory power socket, key interlock solenoid (A/T), Microphone (with navigation) Via passenger's under-dash fuse/relay box: Navigation display unit, Audio unit, Interface dial, Navigation unit (LHD model), HFT/navigation microphone (LHD model), Hands Free Telephone control unit (RHD model)
19 | 20 A | Driver's power seat motors (slide, front up-down), Power seat control unit (with DPMS)
20 | 20 A | Sunroof control unit/motor

*1: | With automatic wiper
*2: | With headlight leveling system (without HID)
*3: | With daytime running lights

Driver's Under-dash Fuse/Relay Box

Fuse Number | Amps | Component(s) or Circuit(s) Protected
--- | --- | ---
21 | 20 A | Driver's power seat motor (recline, rear up-down), Power seat control unit (with DPMS)
22 | 20 A | Driver's MICU, Left rear power window switch (with all power windows AUTO UP/AUTO DOWN function) (LHD model), Left rear power window switch (without all power windows AUTO UP/AUTO DOWN function) (LHD model), Right rear power window switch (with all power windows AUTO UP/AUTO DOWN function) (RHD model), Right rear power window switch (without all power windows AUTO UP/AUTO DOWN function) (RHD model)
23 | 20 A | Accessory power socket relay
24 | 20 A | Door multiplex control unit (Power window master switch)
25 | 15 A | Driver's door lock actuator, Trunk lid release actuator, Driver's MICU, Fuel fill door lock actuator, Left rear door lock actuator (LHD model), Diode (LHD model), Right rear door lock actuator (RHD model)
26 | 10 A | Driver's MICU, Left front fog light (LHD model), Right front fog light (RHD model)
27 | 10 A | Driver's MICU, License plate light, Left taillight, Right taillight, Left front position light (LHD model), Right front position light (RHD model)
28 | 10 A | Driver's MICU (H/L HI)
29 | 10 A *3 | Daytime running lights relay, Front position lights, Taillights, License plate lights
30 | 15 A | Driver's MICU (H/L LO)
31 | ——— | Not used

*3: | With daytime running lights