( TL19E1QE10436455079KBAT00 )

A/T Interlock System - Shift Lock Release, Release Spring, and Release Shaft Replacement

NOTE: This replacement applies for the LHD model.

1. Remove the shift lever assembly.

1. Remove the shift lever knob.

1. Remove the shift lever boot and the A/T gear position indicator panel base.

1. Release the lock (A) of the shift lock release (B), then remove the shift lock release and the release spring (C).

1. Release the lock (D) of the shift lock release shaft (E), and remove the release shaft.

1. Replace the shift lock release, the release spring, or the release shaft.