( TL19E00J26273450001KDAT00 )

Interior Trim Removal/Installation - Rear Shelf Area

1. Remove the rear shelf (A). Be careful not to damage the speakers.

   -1. | Using a clip remover, detach the clips.
   -2. | Lift the rear shelf upward and forward to release the rear hook (B) from the body.
   -3. | Slightly warp the rear shelf to release both side edges from the side curtain airbag inflators, then pull it forward.

1. Install the shelf in the reverse order of removal, and note these items:
   - Using a clip remover, remove any clips left in the body, and reinstall them on the rear shelf.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Be careful no to damage the speakers.
   - When installing the rear bulkhead cover, slip the rear seat belt through the slits, and pass the rear center seat belt through the hole in the cover properly.
   - Push the clips and the hooks into place securely.
   - Make sure the high mount brake light socket is connected securely.