( TL19E00J36100040151KDAT01 )

HFT/Navigation Microphone Removal/Installation - With NAV.

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the dashboard and related parts.
- Lay a workshop towel under the parts when working on them to protect the face panel from scratches or other damage.

1. Remove the roof console.

1. Remove the screws and the HFT/navigation microphone (A).

1. Disconnect the connectors (B) from the roof console.

1. Install the HFT/navigation microphone in the reverse order of removal.