( TL19E00J16126721401KDAT00 )

Front Door Panel Removal/Installation

1. Install the door panel in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Replace any damaged cable fasteners with new ones.
   - The latch cable (A) should be fixed to the cable fastener (B) with the latch in the unlocked position as shown.
   - Make sure the connectors are plugged in properly, and the cables are connected securely.
   - Make sure the window and power door lock operate properly.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.