( TL19E00J46643461354FHAT20 )

Inclination Sensor OFF Switch Test/Replacement

1. Remove the driver's dashboard undercover, then remove the driver's dashboard lower cover.

1. Disconnect the 13P connector from the inclination sensor OFF switch (A), then remove the switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity check is not as specified, replace the illumination bulbs (B) or the switch.