( TL19E00J16166220361KBAT00 )

Rear Door Glass Outer Weatherstrip Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the door.
- Take care not to damage the front hook in the weatherstrip because it is not able to replace with a new one.

1. Remove these items:
   - Door panel
   - Door panel bracket
   - Plastic cover, as needed

1. Raise the glass fully.

1. From the inside of the door, slide the clips (A) of the door glass outer weatherstrip (B) to release the hooks (C) from the flanges (D) of the door panel.