( TL19E00K75100081040FAAT00 )

DTC Troubleshooting: 4

1. Check for continuity between LKAS control unit 26P connector No. 6 terminal and steering angle sensor 5P connector No. 3 terminal.

Is there continuity?

YES | - | Go to Step 18 .
NO | - | Repair an open in the wire between the LKAS control unit and the steering angle sensor.■

1. Check for VSA modulator-control unit DTCs with HDS.

Are any DTCs indicated?

YES | - | Troubleshoot the VSA modulator-control unit DTC(s).■
NO | - | Check for loose terminals in the LKAS control unit connector, and repair if necessary. If all connections are OK, replace the LKAS control unit. ■