( TL19E1PE10410417258KBAT00 )

Torque Converter Housing Selector Control Shaft Oil Seal Replacement

Special Tools Required
Driver handle 15 x 135L
07749-0010000
Oil seal driver attachment
07947-ZV00100

1. Remove the oil seal (A) from the torque converter housing (B).

1. Install a new oil seal (A) in the torque converter housing to a depth (B) of 0.5−1.5 mm (0.02−0.06 in.) below the torque converter housing surface using the 15 x 135L driver handle and the oil seal driver attachment.