( TL19E00K77C000Y2629FAAT00 )

DTC Troubleshooting: B2629

DTC B2629:
Left Rear Corner Parking Sensor Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2629 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Turn the ignition switch to LOCK (0).

1. Swap the left rear corner parking sensor and the left rear center parking sensor.

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2629 indicated?

YES | - | Go to Step 8 .
NO | - | Replace the left rear corner parking sensor.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 6P connector from the left rear corner parking sensor.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the left rear corner parking sensor 6P connector No. 6 terminal and body ground.

Is there about 8 V?

YES | - | Go to Step 12 .
NO | - | Go to Step 22 .

1. Turn the ignition switch to LOCK (0).

1. Check for continuity between the left rear corner parking sensor 6P connector No. 2 terminal and body ground.

Is there continuity?

YES | - | Go to Step 14 .
NO | - | Repair an open in the wire.■

1. Disconnect the 16P connector from the parking and back-up sensor control unit.

1. Connect the parking and back-up sensor control unit 16P connector No. 11 terminal and body ground with a jumper wire.

1. Check for continuity between the left rear corner parking sensor 6P connector No. 4 terminal and body ground.

Is there continuity?

YES | - | Go to Step 17 .
NO | - | Repair an open in the wire.■

1. Remove the jumper wire from the parking and back-up sensor control unit.

1. Check for continuity between the left rear corner parking sensor 6P connector No. 4 terminal and body ground.

Is there continuity?

YES | - | Repair a short to ground in the wire.■
NO | - | Go to Step 19 .

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2632 also indicated?

YES | - | Go to the DTC B2632 troubleshooting.■
NO | - | Replace the parking and back-up sensor control unit .■

1. Measure the voltage between the left rear corner parking sensor 6P connector No. 6 terminal and body ground.

Is there battery voltage?

YES | - | Repair a short to power in the wire.■
NO | - | Go to Step 23 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 16P connector from the parking and back-up sensor control unit.

1. Connect the parking and back-up sensor control unit 16P connector No. 12 terminal and body ground with a jumper wire.

1. Check for continuity between the left rear corner parking sensor 6P connector No. 6 terminal and body ground.

Is there continuity?

YES | - | Replace the parking and back-up sensor control unit .■
NO | - | Repair an open in the wire.■