( TL19E00H46400012803KBAT00 )

Front Passenger's Airbag Replacement

Removal
NOTE: If the front passenger's airbag has been deployed, refer to the install for after a collision where the front passenger's airbag deployed.

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the glove box.

1. Disconnect the dashboard wire harness 4P connector (A) from front passenger's airbag.