( TL19E00D14313514741FEAT00 )

Brake Fluid Level Switch Test

1. Disconnect the brake fluid level switch connector.

1. Check for continuity between the terminals (1) and (2) with the float in the down position and in the up position.
   NOTE:
   - Remove the brake fluid completely from the reservoir. With the float down, there should be continuity.
   - Fill the reservoir with brake fluid to the MAX (upper) level (A). With the float up, there should be no continuity.
   - If both the ABS/VSA indicator and the brake system indicator come on at the same time, check the VSA system first.
   - If the parking brake switch and brake fluid level switch are OK, but the brake system indicator does not function, do the gauge control module test.

1. Reconnect the brake fluid level switch connector.