( TL19E00J18526327895KBAT00 )

Fuel Fill Door Adapter Replacement

1. If necessary, remove the grommet (A) from the body.

   -1.

   Remove the left trunk side trim panel:
   - With temporary repair kit (TRK)/with compact spare tyre
   - With normal spare tyre

   -2. | From trunk compartment, pinch the hooks (B), then remove the grommet by releasing the seal (C) from the body.
   -3. | Pull the grommet out from the rod (D) of the fuel fill door actuator.