( TL19E20A20326428302FAAT00 )

Fuel Pump Circuit Troubleshooting

1. Check for continuity between driver's under-dash fuse/relay box connector F (33P) terminal No. 31 to body ground.

Is there continuity?

YES

-

- Replace PGM-FI main relay 1 .■
- If needed, replace the driver's under-dash fuse/relay box. ■

NO

-

- Repair open in the wire between under-hood fuse relay box and driver's under-dash fuse/relay box.■
- If needed, replace the under-hood fuse/relay box. ■