( TL19E20A14400049001KBAT00 )

Radiator Replacement

1. Connect the fan motor connectors (A) and ECT sensor 2 connector (B), then install the harness clamp (C).

1. Install the lower radiator hose (D).

1. A/T model: Install the ATF cooler hoses (E).

1. Install the splash shield.

1. Lower the vehicle on the lift.

1. Refill the radiator with engine coolant, and bleed the air from the cooling system with the heater valve open.

1. Clean up any spilled engine coolant.