( TL19E00J34200057266KBAT00 )

Sunroof Frame and Drain Tube Replacement

1. Install the frame and the drain tube in the reverse order of removal, and note these items:
   - Before installing the frame, clear the drain tubes and the drain valves using compressed air.
   - When installing, tie the string that was left in the pillar to the top end of the new drain tube and pull it up into the roof.
   - Check the frame seal.
   - Clean the surface of the frame.
   - When installing the frame, first attach the rear hooks into the body holes.
   - Make sure the connectors are plugged in properly.
   - When connecting the drain tube, slide it over the frame nozzle at least 10 mm (0.39 in.).
   - Install the tube clip (A) on the drain tube (B) as shown.
   - After all parts are installed, including the headliner, reset the sunroof control unit.
   - Do the glass position alignment procedure.

1. Check for water leaks. Let the water run freely from a hose without a nozzle. Do not use a high-pressure spray.