( TL19E00J54460647103FEAT00 )

Power Window Front Passenger's Motor Test

Motor Test

1. Remove the front passenger's power window switch.

1. Test the motor in each direction by connecting battery power and ground to the front passenger's power window switch 37P connector (A) according to the table.

1. If the motor does not run or fails to run smoothly, go to Step 4 , if the motor runs smoothly, go to Step 8 .

1. Remove the door panel.