( TL19E00J32133114883KBAT00 )

Exterior Light Bulb Replacement

1. Disconnect the 1P connector (A) from the headlight bulb (B).

   Headlight Bulb (Low Beam): | 55 W

1. Pull the retaining spring (C) away from the bulb then remove the bulb.

1. Install a new bulb in the reverse order of removal. Make sure the notches in the bulb align with the tabs in the headlight.
   NOTE: Do not touch the glass of the bulb with your hands. If necessary, clean the glass area with alcohol.