( TL19E00J10300013233KDAT00 )

Audio/Navigation Switch Panel Removal/Installation

With Navigation System
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the dashboard and related parts.
- Lay a workshop towel under the parts when working on them to protect the face panel from scratches or other damage.
- Do not work in a dusty or dirty place.
- Discharge static electricity from your body before and during the work.
- Do not touch the circuit board with your bare hands.
- Do not work with dirty hands.
- Be careful not to fold the flat plate cable.
- Do not touch the terminal connector of the flat plate cable with your bare hands. (If you have touched it, wipe it off thoroughly.)

1. Remove these items:
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Climate control unit

1. Remove pull out the audio/navigation switch panel (A).

1. Disconnect the connectors (B), and remove the audio/navigation switch panel.

1. Remove the dashboard center vent.

1. Remove the interface dial and hazard switch from the audio/navigation switch panel (A).

1. Install the audio/navigation switch panel in the reverse order of removal.