( TL19E00J54400065501KBAT00 )

Windshield Replacement

1. Attach the rubber dam B with adhesive tape to the inside surface of the windshield (A) as shown.
   - Be sure the rubber dam lines up with the alignment marks (C).
   - With the edge (D) of the black ceramic on the windshield as a guide, attach the rubber dam B to the windshield.
   - Be careful not to touch the windshield where adhesive will be applied.

   Rubber dam adhesive tape:
   | Thickness 0.16 mm (0.006 in.)
   | Width 3.5 mm (0.14 in.)