( TL19E00J34600041953FCAT00 )

MICS (Driver's MICU, Passenger's MICU, and Door Multiplex Control Unit) Input Test

Door Multiplex Control Unit

1. Turn the ignition switch to LOCK (0), open and close the driver's door, then remove the power window master switch.

1. Disconnect the 37P connector (A) from the door multiplex control unit (B).
   NOTE: The illustration shows LHD model.

1. Inspect the connector and socket terminals to be sure they are all making good contact.
   - If the terminals are bent, loose, or corroded, repair them as necessary and recheck the system.
   - If the terminals look OK, go to Step 14 .

1. With the connector still disconnected, and make these input tests at the connector.
   - If any test indicates a problem, find and correct the cause, then recheck the system.
   - If all the input test prove OK, go to Step 15 .

   Cavity | Wire | Test condition | Test: Desired result | Possible cause if desired result is not obtained
   --- | --- | --- | --- | ---

   32

   BLK

   Under all conditions

   Check for continuity to ground: There should be continuity.

   - Poor ground (G501)
   - An open in the wire

   37

   BLK

   Under all conditions

   Check for continuity to ground: There should be continuity.

   - Poor ground (G502)
   - An open in the wire

   13

   WHT

   Under all conditions

   Measure the voltage to ground: There should be battery voltage.

   - Blown No. 15 (10 A) fuse in the under-hood fuse/relay box
   - Faulty driver's under-dash fuse/relay box
   - An open in the wire

1. If multiple failures are found on more than one control unit, replace the driver's under-dash fuse/relay box (includes the driver's MICU). If input failures are related to a particular control unit, replace the control unit.