( TL19E00K733000Y1241FAAT00 )

DTC Troubleshooting: B1241 (N and A/C ON)

1. Measure the voltage between the blower motor 2P connector No. 1 terminal and body ground.

Is there battery voltage?

YES | - | Replace the blower motor.■
NO | - | Go to Step 28 .

1. Turn the ignition switch to LOCK (0).

1. Remove the blower motor relay from the under-hood fuse/relay box, and test it.

Is the relay OK?

YES | - | Go to Step 30 .
NO | - | Replace the blower motor relay .■