( TL19E00J4616645402QKBAT00 )

Rear Seat Release Lever Replacement

1. Disconnect the rear seat-back release cable (A). Take care not to kink the cable.

1. Install the release lever in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Make sure the release cable is connected securely.
   - Make sure the seat-back locks securely and unlocks properly.