( TL19E00D52100063635KDAT00 )

VSA Modulator-control Unit Removal and Installation

1. Disconnect the VSA modulator-control unit 47P connector (A) by pushing the lock (B) and pulling down the lever (C); the connector disconnects itself.

1. Disconnect the six brake lines from the VSA modulator-control unit.
   NOTE: Brake lines are connected to the master cylinder (D) and to the left-front (E), the right-front (F), the left-rear (G), and the right-rear (H) brake systems.

1. Remove the 6 x 12 mm flange bolts (I) and 6 x 16 mm flange bolt (J), then remove the VSA modulator-control unit (K) with the bracket (L) from the body.

1. Remove the receiver line (M) from the bracket, then remove the clips (N).

1. Remove the VSA modulator-control unit from the bracket.