( TL19E00J54226561995DCAT00 )

Under-dash Fuse/Relay Box (Driver's) Connector Locations

Driver's Under-dash Fuse/Relay Box

Socket | Ref | Terminal | Connects to | Notes
--- | --- | --- | --- | ---
A | 1 | ——— | Not used |
B | 2 | 2 | Dashboard wire harness [Not used] |
C | 3 | 5 | Dashboard wire harness |
Cigarette lighter relay | 4 | 4 |  |
D | 11 | 16 | Left [right] side wire harness |
E | 10 | 20 | Left [right] side wire harness |
F | 9 | 33 | Left engine compartment wire harness |
G | 8 | 13 | Left engine compartment wire harness |
H (optional connector) | 7 | 12 | Not used |
K (MICU service check connector) | 6 | 3 |  |
M | 13 | 4 | Dashboard wire harness |
N | 14 | 16 | Dashboard wire harness |
P | 15 | 20 | Dashboard wire harness |
PGM-FI main relay 2 (FUEL PUMP) | 12 | 4 |  |
Q | 17 | 20 | Dashboard wire harness |
R | 16 | 24 | Dashboard wire harness |
Starter cut relay | 5 | 4 |  |

[ ]: | RHD model