( TL19E00J34600000000CAAT00 )

Keyless Entry System (Unlock only driver's door first, then other doors and trunk lid)
The driver's MICU controls the door lock actuators based upon the input signals of each switch.

| Input | Output
--- | --- | ---
Driver's MICU | IG1 power supply Ignition key switch Driver's door switch Left [right] rear door switch Trunk lid opener main switch | Door lock actuators (LOCK) Driver's door lock actuator (UNLOCK) Door lock actuators (UNLOCK) Trunk lid release actuator

B-CAN

Front passenger's door switch
Right [left] rear door switch
Driver's door lock knob switch (LOCK)
Driver's door lock switch (LOCK/UNLOCK)
Driver's door key cylinder switch (LOCK/UNLOCK)
Front passenger's door lock switch (LOCK/UNLOCK)
Keyless LOCK/UNLOCK signal

Door lock (LOCK) signal
Door lock (UNLOCK) signal
Relock signal

[ ]: | RHD model