( TL19E00F00000057101KDAT00 )

Steering Column Removal and Installation

1. Disconnect the wire harness connectors from the combination switch assembly/cable reel (A).

1. Remove the combination switch assembly from the steering column shaft by removing the three screws (B).

1. Disconnect the connectors from the ignition switch, and release the wire harness clips from the steering column.

1. Remove the steering column (C) by removing the attaching nuts and bolts.