( TL19E00J34300044021KBAT00 )

Mirror Holder Replacement

NOTE: Put on gloves to protect your hands.

1. Carefully push on the top edge of the mirror holder (A) by hand.

1. Put a shop towel in the opening between the bottom edge of the mirror holder and the mirror housing (B) to prevent scratches. Insert a flat-tip screwdriver wrapped with protective tape to the guide notches (C) of the mirror holder, and detach the bottom clips (D).