( TL19E00J36100000000FEAT00 )

Navigation System Diagnostic Mode

Icon Color Information

Icon | Icon Color
--- | ---
GREEN | RED | YELLOW | WHITE | GRAY
Display | Result of ‘‘Connection'' under the ‘‘Display'' diagnosis menu is OK. | Result of ‘‘Connection'' under the ‘‘Display'' diagnosis menu is NG. | ——— | Executing (Not completed) | ———
Radio | Result of ‘‘Connection'' under the ‘‘Radio'' diagnosis menu is OK. | Result of ‘‘Connection'' under the ‘‘Radio'' diagnosis menu is NG. | ——— | Executing (Not completed) | ———
GPS Ant. | All result of ‘‘Antenna'' and ‘‘Receiver in NAVI ECU'' is OK. | Any result of ‘‘Antenna'' and ‘‘Receiver in NAVI ECU'' is OK. | ——— | Executing (Not completed) | ———
R-Camera | Result of ‘‘Connection'' under the ‘‘R-Cammera'' diagnosis menu is OK. | Result of ‘‘Connection'' under the ‘‘R-Cammera'' diagnosis menu is NG. | ——— | Executing (Not completed) | ———
TMC Ant. | All result of ‘‘Antenna'' and ‘‘Receiver in NAVI ECU'' is OK. | Any result of ‘‘Antenna'' and ‘‘Receiver in NAVI ECU'' is OK. | ——— | Executing (Not completed) | ———
A/C | Result of ‘‘Connection'' under the ‘‘Aircon'' diagnosis menu is OK while ‘‘Ignition'' is ON. | Result of ‘‘Connection'' under the ‘‘Aircon'' diagnosis menu is NG while ‘‘Ignition'' is ON. | While ‘‘Ignition'' is OFF. | Executing (Not completed) | ———
Meter (F-CAN) | All result of F-CAN related units are OK. | Any result of F-CAN related units are NG. | ——— | Executing (Not completed) | ———
HFT | Result of ‘‘Connection'' under the ‘‘HFT'' diagnosis menu is OK. | Result of ‘‘Connection'' under the ‘‘HFT'' diagnosis menu is NG. | ——— | Executing (Not completed) | ———
Mic | The microphone detects the sound ‘‘Pi-Pi-Pon'' at the system link menu. | The microphone could not detects the sound ‘‘Pi-Pi-Pon'' at the system link menu. | ——— | Executing (Not completed) | ———
ECU Info. | Both V-RAM or D-RAM is OK, and all ‘‘Program Flash'', ‘‘Serial No.'', ‘‘Model'' is available, and the DVD lid is closed. | Either the V-RAM or D-RAM is NG, or any of the ‘‘Program Flash'', ‘‘Serial No.'', ‘‘Model'' is unavailable. | DVD lid is opened | Executing (Not completed) | ———
Hard Key | All buttons are pressed and are detected under ‘‘Hard key'' menu. | All buttons are not pressed or pressed but not detected under ‘‘Hard key'' menu, or exit from ‘‘Hard key'' menu without the button not detected. | ——— | ——— | Until changing to ‘‘Hard key'' menu.
Error History | ——— | ——— | ‘‘Hard Error'' or ‘‘Soft Error'' is detected under ‘‘Error History'' menu. | Executing (Not completed) | ‘‘Hard Error'' or ‘‘Soft Error'' is not detected under ‘‘Error History'' menu.
DVD | DVD mechanism is normal and the proper DVD is installed. | ——— | Improper DVD is installed, or DVD is not installed, or can not identify software version from the DVD or internal mechanism failure. | Executing (Not completed) | ———
Yaw Sensor | Result of the ‘‘Yaw Sensor'' diagnosis menu is OK. | Result of the ‘‘Yaw Sensor'' diagnosis menu is NG. | Result of the ‘‘Zero Point Output'' under the ‘‘Yaw Sensor'' diagnosis menu is NO CHECK. | Executing (Not completed) | ———
Car Status | ——— | ——— | ——— | ——— | Check these systems manually.