( TL19E1AE34116300000BAAT00 )

Clutch Hydraulic System Bleeding

1. Attach the one end of a clear tube to the bleeder screw (A), and put the other end into a container of brake fluid. Loosen the bleeder screw to allow air to escape from the system.

1. Make sure there is an adequate supply of fluid in the reservoir, then slowly pump the clutch pedal until no more bubbles appear at the clear tube.
   NOTE: Temporary tighten the bleeder screw when clutch pedal is returned.

1. Tighten the bleeder screw securely.

1. Refill the brake fluid in the reservoir to the MAX (upper) level line.

R20A3 engine model
K24Z3 engine model