( TL19E1PE10411354202KBAT00 )

Torque Converter Housing Secondary Shaft Bearing Replacement

1. Install the secondary shaft bearing securely in the torque converter housing using the 15 x 135L driver handle and the 62 x 68 mm bearing driver attachment.

1. Check that the bearing groove aligns with the torque converter housing surface, then install the bearing set plate with aligning the bearing groove.

1. Install a new lock washer and bolt, then bend the lock tab of the lock washer against the bolt head.