( TL19E20A18316600000KCAT00 )

Crankshaft/Oil Seal (Transmission End) Installation

1. Seat the rod journals into connecting rod No. 1 and connecting rod No. 4. Line up the mark (A) on the connecting rod and the cap, then install the caps and the bolts finger-tight.

1. Rotate the crankshaft clockwise, and seat the journals into connecting rod No. 2 and connecting rod No. 3. Line up the mark on the connecting rod and the cap, then install the caps and the bolts finger-tight.

1. Tighten the connecting rod bolts to 20 N·m (2.0 kgf·m, 14 lbf·ft).