( TL19E00E16226600000LCAT00 )

Driveshaft Disassembly

Special Tools Required
Threaded adapter, 26 x 1.5 mm
07XAC-0010300
Sliding hammer set
07936-5790002
Puller, commercially available
Boot band pliers, commercially available
Inboard Joint Side

1. Remove the boot bands. Be careful not to damage the boot.
   - If the boot band is a welded type (A), cut the boot band.
   - If the boot band is a double loop type (B), lift up the band end (C), and push it into the clip (D).
   - If the boot band is a low profile type (E), pinch the boot band using commercially available boot band pliers (F).

Welded type
Double loop type
Low profile type