( TL19E1PE10410424251KCAT00 )

A/T End Cover Installation

1. Install new conical spring washers (A) with facing stamped mark side up in the direction shown, and install a new mainshaft locknut (B), a new countershaft locknut (C), and a new secondary shaft locknut (D).

1. Tighten the locknuts to 167 N·m (17.0 kgf·m, 123 lbf·ft).
   NOTE:
   - Be sure to install the conical spring washers in the direction shown.
   - Use a torque wrench to tighten the locknut. Do not use an impact wrench.
   - Countershaft and secondary shaft locknuts have left-hand threads.

1. Remove the spline shaft holder set from the mainshaft.