( TL19E00K791000R8561FAAT00 )

DTC Troubleshooting: 85-61, 85-62

1. Measure the voltage between the No. 1 terminal of the SRS unit connector B (39P) and body ground. There should be 0−0.05 V.

Is there battery voltage?

YES | - | Go to Step 16 .
NO | - | Short to power between the No. 1 terminal of the SRS unit connector B (39P) and the No. 7 terminal of the OPDS unit harness 18P connector (dashboard wire harness, right side wire harness, SRS floor wire harness, or OPDS unit harness); replace the faulty harness.■

1. Replace the OPDS unit.

1. Clear the DTC.

1. Read the DTC.

Is the DTC 85-61 or 85-62 indicated?

YES | - | Replace the SRS unit. ■
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.