( TL19E00J10300013145FEAT00 )

Audio Remote Switch Test

1. Remove the audio remote switch.

1. Measure the resistance between the terminals No. 7 and No. 9 in each switch position according to the table.

   Position | Resistance
   --- | ---
   OFF | About 10 kΩ
   MODE | About 3.7 kΩ
   CH (+) | About 1.7 kΩ
   CH (−) | About 775 Ω
   ▲ (VOL.UP) | About 357 Ω
   ▼ (VOL.DOWN) | About 100 Ω

1. If the resistance is not as specified, replace the audio remote switch.