( TL19E00J54460647105FEAT02 )

Power Window Rear Motor Test - Without All Power Windows AUTO UP/DOWN Function

1. Check for continuity between the rear power window switch 14P connector No. 1 and No. 7 terminals and the rear power window motor 2P connector No. 1 and No. 2 terminals respectively. There should be continuity.

   REAR POWER WINDOWSWITCH 14P CONNECTOR | REAR POWER WINDOWMOTOR 2P CONNECTOR
   --- | ---
   No. 1 terminal | No. 1 terminal
   No. 7 terminal | No. 2 terminal

1. If the wire harness is OK, replace the rear power window motor.