( TL19E00J26273460309KDAT00 )

Interior Trim Removal/Installation - Trunk Lid

Trunk Lid Trim Panel - For Some Models
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the panel.
- When removing components, use the trim tools or equivalent.

1. On both sides, remove the clips fastening the trunk lid hinge trim A, B, and the trunk lid trim panel (C), then separate the upper portions of the trim A and B from the trunk hinge by detaching the hooks (D).