( TL19E00J18513415012KDAT00 )

Rear Bumper Removal/Installation

1. With the help of an assistant, pull the rear bumper to release the bumper (A) from the hooks (four places) (B) on the upper brackets (C). With rear corner sensors and back sensors: While holding the bumper, disconnect the rear bumper corner sensor subharness connector (D).

1. Install the bumper in the reverse order of removal, and note these items:
   - If equipped, make sure the rear bumper corner sensor subharness connector is plugged in properly.
   - Make sure the rear bumper engages the hooks (of both side spacers and rear spacers) on each side securely.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hooks into place securely.